|  |  |  |
| --- | --- | --- |
| Company Name | Phone | Fax |
|  |  |  |
| Contact person | Address | |
|  |  | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Product | Rubber | Metal | | Nonwoven | | Plastics | | |
| PU/PUR  polyurethane | GRP/CRP  Composite | | Mineral Casting | | | | |
| Your Industry | Automotive  Supplier | Rubber to  metal bonding | | Aerospace  Industry | | Furniture  Industry | | |
| Pharmaceutical | Tire Industry | | Shoes  industry | | Technical  Components | | |
| Wind Power | Metal  Processing | | Model and mold  construction | | | | |
| The Molding materials | Iron | Stainless Steel | | Aluminum | | | | |
| Epoxy Resin | Vinyl Resin | | Other | | | | |
| Product base materials | Epoxy Resin | Methacrylate | | Carbon Fiber | | | | |
| Fiber glass | Other | | | | | | |
| Curing Temperature | Below 20°C | 20°C-60°C | | 61°C-150°C | | | 180°C  above | |
| Curing Time | 30 Minutes | 1 hour | | 1-2 hours | | | | |
| 2-3 hours | Other | | | | | | |
| Mold Release agent | Wax | PMR | | Other | | | | |
| Sealants | Need | No Need | | Will consider | | | | |
| Number of mold release | 1 times | 3-5 times | | 5-8 times | | | | |
| 20 times | 40 times | | 40 times above | | | | |
| Problem occur during molding | Degree of Finish | Few times of mold release | | Molding time takes too long | | | | |
| Hard to release | Surface treatment need after mold release | | Operation trivial | | | | Other |
| Product requirement | Good Brightness | One time processing | Secondary Processing | | None Transfer | | | |
| Note |  | | | | | | | |