|  |  |  |
| --- | --- | --- |
| Company Name | Phone  | Fax |
|  |  |  |
| Contact person | Address |
|  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Product | [ ]  Rubber | [ ]  Metal | [ ]  Nonwoven | [ ]  Plastics |
| [ ]  PU/PUR  polyurethane | [ ]  GRP/CRP  Composite | [ ]  Mineral Casting |
| Your Industry | [ ]  Automotive  Supplier | [ ]  Rubber to  metal bonding | [ ]  Aerospace  Industry | [ ]  Furniture  Industry |
| [ ]  Pharmaceutical | [ ]  Tire Industry | [ ]  Shoes  industry | [ ]  Technical Components |
| [ ]  Wind Power | [ ]  Metal  Processing | [ ]  Model and mold  construction |
| The Molding materials | [ ]  Iron | [ ]  Stainless Steel | [ ]  Aluminum |
| [ ]  Epoxy Resin | [ ]  Vinyl Resin | [ ]  Other |
| Product base materials | [ ]  Epoxy Resin | [ ]  Methacrylate | [ ]  Carbon Fiber |
| [ ]  Fiber glass | [ ]  Other |
| Curing Temperature | [ ]  Below 20°C | [ ]  20°C-60°C | [ ]  61°C-150°C | [ ]  180°C  above |
| Curing Time | [ ]  30 Minutes | [ ]  1 hour | [ ]  1-2 hours |
| [ ]  2-3 hours | [ ]  Other |
| Mold Release agent | [ ]  Wax | [ ]  PMR | [ ]  Other |
| Sealants | [ ]  Need | [ ]  No Need | [ ]  Will consider |
| Number of mold release | [ ]  1 times | [ ]  3-5 times | [ ]  5-8 times |
| [ ]  20 times | [ ]  40 times | [ ]  40 times above |
| Problem occur during molding | [ ]  Degree of Finish | [ ]  Few times of mold release | [ ]  Molding time takes too long |
| [ ]  Hard to release | [ ]  Surface treatment need after mold release | [ ]  Operation trivial | [ ]  Other |
| Product requirement | [ ]  Good Brightness | [ ]  One time processing | [ ]  Secondary Processing | [ ]  None Transfer |
| Note |  |